



点击USB 鼠标右键更新驱动程序进入下一个界面


Click Right button of mouse on “my computer” to open the device manager as above,**turn off the watch, then connect the cable to the turn-off status watch**, sometimes it will prompt “install USB driver”, sometimes it prompts “unknow device” in the device manager. If it is a yellow exclamation mark, click right key of mouse and go to renew driver as above.




Click next step

****


Select the location of driver



**Click the “browse” button, select the location where the driver is, select win7 fold if on windows 7 or select “2KXP COM ” on windows xp**

****

**Keep going on**

****

**Finish the driver installation, need to do it again if change to another computer**